.encoding = "windows-1252"
config.version = "8"
virtualHW.version = "11"
scsi0.present = "TRUE"
scsi0.virtualDev = "lsilogic"
memsize = "512"
ide0:0.present = "TRUE"
ide0:0.fileName = "pfSense.vmdk"
ide1:0.present = "TRUE"
ide1:0.autodetect = "TRUE"
ide1:0.deviceType = "cdrom-raw"
ethernet0.present = "TRUE"
ethernet0.connectionType = "nat"
ethernet0.virtualDev = "e1000"
ethernet0.wakeOnPcktRcv = "FALSE"
ethernet0.addressType = "generated"
ethernet0.pciSlotNumber = "33"
ethernet0.generatedAddress = "00:0c:29:55:d3:08"
ethernet0.generatedAddressOffset = "0"
ethernet1.present = "TRUE"
ethernet1.vnet = "VMnet16"
ethernet1.connectionType = "custom"
ethernet1.virtualDev = "e1000"
ethernet1.wakeOnPcktRcv = "FALSE"
ethernet1.addressType = "generated"
ethernet1.pciSlotNumber = "37"
ethernet1.generatedAddress = "00:0c:29:55:d3:12"
ethernet1.generatedAddressOffset = "10"
usb.present = "TRUE"
ehci.present = "TRUE"
ehci.pciSlotNumber = "35"
sound.present = "TRUE"
sound.fileName = "-1"
sound.autodetect = "TRUE"
pciBridge0.present = "TRUE"
pciBridge4.present = "TRUE"
pciBridge4.virtualDev = "pcieRootPort"
pciBridge4.functions = "8"
pciBridge5.present = "TRUE"
pciBridge5.virtualDev = "pcieRootPort"
pciBridge5.functions = "8"
pciBridge6.present = "TRUE"
pciBridge6.virtualDev = "pcieRootPort"
pciBridge6.functions = "8"
pciBridge7.present = "TRUE"
pciBridge7.virtualDev = "pcieRootPort"
pciBridge7.functions = "8"
vmci0.present = "TRUE"
hpet0.present = "TRUE"
displayName = "pfSense"
guestOS = "freebsd"
nvram = "pfSense.nvram"
virtualHW.productCompatibility = "hosted"
powerType.powerOff = "soft"
powerType.powerOn = "soft"
powerType.suspend = "soft"
powerType.reset = "soft"
extendedConfigFile = "pfSense.vmxf"
ide1:0.fileName = "auto detect"
numa.autosize.vcpu.maxPerVirtualNode = "1"
numa.autosize.cookie = "10001"
uuid.bios = "56 4d 82 1a b3 f6 c1 99-7d 5d fe f0 e4 55 d3 08"
uuid.location = "56 4d 42 e8 eb 92 cc 79-b8 6d c9 46 bb 1c e3 73"
uuid.action = "keep"
migrate.hostlog = ".\pfSense-e4b4b008.hlog"
ide0:0.redo = ""
pciBridge0.pciSlotNumber = "17"
pciBridge4.pciSlotNumber = "21"
pciBridge5.pciSlotNumber = "22"
pciBridge6.pciSlotNumber = "23"
pciBridge7.pciSlotNumber = "24"
scsi0.pciSlotNumber = "16"
usb.pciSlotNumber = "32"
sound.pciSlotNumber = "34"
vmci0.pciSlotNumber = "36"
vmci0.id = "-464137464"
monitor.phys_bits_used = "42"
vmotion.checkpointFBSize = "33554432"
vmotion.checkpointSVGAPrimarySize = "33554432"
cleanShutdown = "TRUE"
softPowerOff = "TRUE"
usb:1.speed = "2"
usb:1.present = "TRUE"
usb:1.deviceType = "hub"
usb:1.port = "1"
usb:1.parent = "-1"
tools.remindInstall = "FALSE"
ide1:0.startConnected = "FALSE"
annotation = "       ====  pfSense 2.2.4 32Bit ====|0D|0A- VMnet 16 == pfSense LAN|0D|0A- pfSense defaults:|0D|0A   - username: admin|0D|0A   - password: pfsense|0D|0A   - DHCP is enabled|0D|0A   - pfSense LAN IP = 192.168.1.1|0D|0A   - pfSense WAN = DHCP client|0D|0A|0D|0AHow to configure:|0D|0A  - Just put a system behind the pfSense router by connecting a VM to VMnet 16 and surfing to http://192.168.1.1"
floppy0.present = "FALSE"
msg.autoAnswer = "TRUE"
answer.msg.uuid.altered = "I copied it"
usb:0.present = "TRUE"
usb:0.deviceType = "hid"
usb:0.port = "0"
usb:0.parent = "-1"
